**Unosim gsm alarm dialer caller**




Figure Board

Dx bus digital inputs\outputs:

Configuration mode pin = D4 

Activation: Connect to ground.

Use for configuration board by special “Unosim configuration tool”.

If pin connected to ground – Configuration mode activated.

If pin not connected to ground – Configuration mode inactivated.

Security input = D5 

Activation: Connect to ground.

Configuration of modes in “Unosim configuration tool”.

SMS pin for receiving status of alarm on or off. Possible enter own text of sms.

If pin connected to ground – sending alarm ‘On’ message.

If pin not connected to ground – sending alarm ‘Off’ message.

Upgrade firmware = D7 

Activation: Connect to ground.

Configuration of modes in “Unosim configuration tool”.

**1) Please remove GSM module from controller and connect to ground.**

2) Push Reset button.

3)Run “Upgrade firmware” button in “Unosim configuration tool”.

Relay output = D10 

Activation: Connect to ground.

Configuration of modes in “Unosim configuration tool”.

Relay output pin for relay. If incoming call from authorized callers (users from Alarm1 or Alarm2 or Alarm3), relay will connect for 2..10 seconds after the call on device.

Possible enter own delay between 2-10 seconds.

Alarm input = D12 

Activation: Connect to ground.

Configuration of modes in “Unosim configuration tool”.

Possible switch call or/and sms mode.

If pin connected to ground – calling or/and sending message to Alarm1 or Alarm2 or Alarm3 users.

If pin not connected to ground – nothing.

Example of “Configuration mode” D4 activation:




Figure Configuration mode




Figure “Unosim configuration tool”




Figure Update firmware